The data is broken into two datasets due to an interruption in the data feed that occurred when the recording software needed to be rebooted.

Any files labeled with ‘A’s are the data that follows from where the original file was interrupted. ‘A’ files are, generally speaking, measured during the up-cast.