Update #1 - Final Update: The LUT Vendor found that the collector software had failed. The Front Processor and Location Processor servers were rebooted and Maryland 1 GEO Ground Station returned to Normal Operations.

Topic: SARSAT Maryland 1 Geostationary (GEO) Ground Station Offline
Date/Time Issued: September 4, 2018 0830Z
Product(s) or Data Impacted: SARSAT alert data
Date/Time of Initial Impact: September 4, 2018 0653Z
Date/Time of Expected End: September 4, 2018 0808Z
Length of Outage: 1 hour and 15 minutes
Details/Specifics of Change: Maryland 1 GEO Ground Station in Suitland, MD stopped sending 406 MHz alert data. The LUT Vendor has been contacted to investigate the problem.
Impact: Minor-Distress alert detection/reporting timeliness due to the redundancy of the SARSAT GEOLUT system.
Contact Information for Further Information: USMCC Operations usmcc@noaa.gov at 301-817-4576
Web Site(s) for applicable information:N/A

This message was sent by ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.