^M ^M ^M ^M ^M
^M
^M

Update#1 GOES-16 Mode-4 change did not began until 1820Z^M

^M

^M

^M

Topic: GOES-16 and GOES-17 ABI Mode Change

^M

Date/Time Issued: December 04, 2018 1829 UTC

^M

Product(s) or Data Impacted: GOES-16 and GOES-17 ABI Data

^M

Date/Time of Initial Impact: December 4, 2018 1800 UTC

^M

Date/Time of Expected End: December 4, 2018 2200 UTC

^M

Length of Event: 4 hours

^M

Details/Specifics of Change:

^M

On December 4, 2018 at 1800 UTC, the GOES-16 (GOES-EAST) and GOES-17 Advanced Baseline Imagers (ABI) will operate in Continuous Full Disk Mode (mode 4) for 4 hours for testing storage updates. Continuous Full Disk Mode means products will be generated for Full Disk only, every 5 minutes.

^M
^M

This test will be cancelled in the event of a Critical Weather Day declaration prior to the event start.

^M

M-B

^M

Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880

^M

M-B

^M

Web Site(s) for applicable information:

^M

See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.

^M

See https://www.goes-r.gov/spacesegment/abi.html for ABI specific information.

^M

M-B

^M This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.M-BM-B
^M
^M
^M
^M