Topic: SNPP VIIRS and CrIS reset and recovery
Date/Time Issued: July 5, 2018 1945Z
Product(s) or Data Impacted: SNPP VIIRS and CrIS Sensor data
Date/Time of Initial Impact: Jul 5, 2018 1920Z
Date/Time of Expected End: Jul 5, 2018 2300Z
Length of Outage: see details
Details/Specifics of Change:
SNPP VIIRS suffered an uncorrectable error and TMON 37 tripped causing swap of 1394 Bus from side B to side A. At AOS of SVL 34652, the CrIS 1394 bus also showed a reset and the CDP root node will need to be recovered. Engineering team is conducting recovery for the next 3 orbits between 19:20 - 2300, and will affect VIIRS and CrIS data. VIIRS instrument will be safed, reset, and both CrIS and VIIRS will be configured back to operation.
Affected orbits are:
SVL 34652: 19:20 - 19:31: VIIRS safed and recycled, VIIRS placed in Op day and producing all data in all bands, including more data during night.
SVL 34653: 21:02 - 21:15
SVL 34653: 22:43 - 22:58
Additional orbits may be required.
Some data may not transferred to users because it did not meet their timeliness requirements.
C ontact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov and 301-817-3880
Web Site(s) for applicable information: N/A
This message was sent by ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.