Topic:M-BGOES-16 ABIM-BdesertM-BmonitoringM-Bcalibration scan
Date/Time Issued:M-B December 17, 2019 1700Z
Product(s) or Data Impacted:M-BGOES-16 ABI outage and mode change
Date/Time of Initial Impact:M-BDecember 21 2019 1600Z
Date/Time of Expected End:M-BDecember 21, 2019 1610Z
Length of Outage:M-BApproximate 5 minute outage followed by 5 minutes of Continuous Full Disk mode
Details/Specifics of Change:M-BA GOES-16 ABI routineM-BdesertM-BmonitoringM-Bcalibration scan will occur from 1600-1610Z on December 21, 2019 following the schedule below:M-B
ABI calibration scan: 1600-1605Z - No ABI products generated or distributed
ABI Continuous Full Disk Mode (mode 4): 1605-1610Z
ABI 10-minute Flex Mode (mode 6) resumes: 1610Z
Contact Information for Further Information:M-BESPC Operations atM-BESPCOperations@noaa.govM-Bor 301-817-3880
Web Site(s) for applicable information:
SeeM-Bhttps://www.ospo.noaa.gov/Operations/messages.htmlM-Bfor this and other satellite related messages.
This message was sent toM-BESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk atM-BESPCOperations@noaa.govM-Bor (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request