Topic: GOES-17 ABI desert monitoring calibration scan

Date/Time Issued: February 22, 2019 1425 UTC

Product(s) or Data Impacted: GOES-17 ABI outage and mode change

Date/Time of Initial Impact: February 25, 2019 2000 UTC

Date/Time of Expected End: February 25, 2019 2015 UTC

Length of Outage: Approximate 5 minute outage followed by 5 minutes of Continuous Full Disk mode

Details/Specifics of Change:

A GOES-17 ABI routine desert monitoring calibration scan will occur from 2000-2010 UTC on February 25, 2019 following the schedule below: M-B

M-B

ABI calibration scan: 2000-2005 UTC - no ABI products generated or distributed

ABI Continuous Full Disk Mode (mode 4): 2005-2010 UTC

ABI mode 6 resumes: 2010 UTC

M-B

Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880

M-B

Web Site(s) for applicable information:

See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.

This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.M-BM-B