^M ^M ^M ^M ^M
^M Topic: GOES-17 ABI solar calibration scan
^M
^M Date/Time Issued:M-BJuly 19, 2019 1250Z^M ^M

Product(s) or Data Impacted: GOES-17 ABI product outage

^M Date/Time of Initial Impact:M-BJuly 22,M-B2019 1510Z^M
^M Date/Time of Expected End: July 22, 2019 1520Z
^M
^M Length of Outage: Approximately 5 minutes at the end of a period of Continuous Full Disk operations^M
^M Details/Specifics of Change: On July 22, 2019, GOES-17 ABI 10-minute Flex Mode (mode 6) will be replaced with 10 minutes of Continuous Full Disk (mode 4) from 1510-1520 UTC. A GOES-17 ABI solar calibration scan will be performed between 1515-1520 UTC, resulting in an outage of all ABI products. ABI 10-minutes Flex Mode (mode 6) will resume at 1520 UTC. The next Full Disk scan will populate at 1520 UTC.
^M

Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880

^M Web Site(s) for applicable information: See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.
^M
^M This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.^M
^M
^M