^M ^M ^M ^M ^M
^M
^M
^M
^M
^M
^M
^M

Topic: GOES-17 EXIS Cruciform Scan Calibration

^M

^M

^M

Date/Time Issued: November 4, 2019 M-B1215Z

^M

^M

^M

Product(s) or Data Impacted: GOES-17 EXIS and SUVI Product Outage

^M

^M

^M

Date/Time of Initial Impact: November 7, 2019 2023Z^M

^M

^M

^M

Date/Time of Expected End: November 7, 2019 2206Z

^M

^M

^M

Length of Outage: 1 hour 43 minutes

^M

^M

^M Details/Specifics of Change:The GOES-17 EXIS instrument will execute a quarterly Cruciform Scan calibration. . ^M

M-B

^M Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880^L GOES Payload ^M ^M Engineering: 301-817-4409^M

Web Site(s) for applicable^M information: N/A
^M

^M

This message was sent^M from ESPC.Notification@noaa.gov. You^M have been sent this and other notifications because^M you have opted in to receive it. If for any reason,^M you wish to unsubscribe, please contact ESPC Help Desk^M at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it^M may take up to two business days to process your^M unsubscribe request.

^M ^M
^M
^M
^M
^M
^M
^M
^M
^M