^M ^M ^M ^M
^M

^M Topic: GOES-17 ABI desert monitoring calibration scan ^M ^M ^M ^M ^M Date/Time Issued: April 18, 2019 1554Z^M ^M ^M Product(s) or Data Impacted: GOES-17 ABI outage and mode change^M ^M ^M Date/Time of Initial Impact: April 23, 2019 M-B1950Z^M ^M ^M Date/Time of Expected End: April 23, 2019 2000Z^M ^M ^M Length of Outage: Approximate 5 minute outage followed by 5 minutes of Continuous Full Disk mode^M ^M ^M Details/Specifics of Change:^M A GOES-17 ABI routine desert monitoring calibration scan will occur from 1950-2000 UTC on April 23, 2019 following the schedule below: ^M ^M ^M ^M ABI calibration scan: 1950-1955 UTC - no ABI products generated or distributed^M ABI Continuous Full Disk Mode (mode 4): 1955-2000 UTC^M ABI 10-minute Flex Mode (mode 6) resumes: 2000 UTC^M ^M ^M Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880^M ^M ^M Web Site(s) for applicable information:^M See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.^M
^M

This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.

^M ^M
^M
^M