Update #1: The time for the last calibration test and ABI outage is now 1930-1945 UTC instead of 2045-2100 UTC.

M-B

Topic: GOES-17 ABI calibration tests and configuration parameter update

Date/Time Issued: February 7, 2019 2035 UTC

Product(s) or Data Impacted: GOES-17 ABI data outages

Date/Time of Initial Impact: February 11, 2019 1645 UTC

Date/Time of Expected End: February 11, 2019 2100 UTC

Length of Outage: Three outages of 15 minutes each

Details/Specifics of Change:

Two GOES-17 ABI calibration tests and a configuration parameter update will occur on February 11, 2019 following the schedule below and resulting in three, 15-minute data outages. M-B

1645-1700 UTC - calibration test and ABI data outage

1700-1715 UTC - configuration parameter update and ABI data outage

2045-2100 UTC - calibration test and ABI data outage

M-B

If NWS Regions have any operational concerns, please contact the NCEP SDM (301) 683-1500.

M-B

Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880

M-B

Web Site(s) for applicable information:

See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.

This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.M-BM-B