Update #1: JASON-2 came out of Safe Hold Mode 05/22/2019 at ~0900Z. The first Jason-2 pass with usable products was 59049 starting at 1131Z.

Topic: No data was received from Jason-2 on Pass 57827, Jason-2 Satellite is in Safe Hold Mode.
Date Issued: May 22, 2019 1640Z
Product(s) or Data Impacted: Jason-2 OGDRs distributed via DDS and Class users.
Date/Time of Initial Impact: February 16, 2019 1456Z
Date/Time of Expected End: May 22, 2019 0900Z
Length of Event: 94 Days 19 hours
Details/Specifics of Change:

During Jason-2 Rev 57827 (AOS 151910Z), we received indications of Safe Hold Mode. After configuring into low bitrate and bringing up the command carrier, the operator sent JA2_TC_SAFE_MODE_RECOVERY_BEGINNING_part1 to the COP-1 AD side. We did not receive initflag condition indication prior to LOS, so will reaccomplish the SHM checklist during the next support (Rev 57828, AOS 171530Z) and command to the COP-1 BD side. TC groups for Part 1, Part 2, and Emergency Patch were successfully uplinked. Spacecraft is in Safe Mode, AOCS is in BBQP. We expect CNES direction to re-enable FDTM during next support (Rev 57829, AOS 191110).
Contact Information for Further Information: ESPCOperations@noaa.gov at 301-817-3880.

Web Site(s) for applicable information: N/A

This message was sent from ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.