^M ^M ^M ^M ^M
^M

Topic: GOES-17 ABI desert monitoring calibration scan ^M

^M

Date/Time Issued:M-BJuly 19, 2019 M-B1256Z

^M

Product(s) or Data Impacted: GOES-17 ABI outage and mode change

^M

Date/Time of Initial Impact:M-BJuly 22,M-B2019 M-B2000Z

^M

Date/Time of Expected End: July 22, 2019 M-B2010Z

^M

Length of Outage: Approximate 5 minute outage followed by 5 minutes of Continuous Full Disk mode

^M Details/Specifics of Change: A GOES-17 ABI routine desert monitoring calibration scan will occur from 2000-2010 UTC on July 22, 2019 following the schedule below: M-B
^M M-B
^M ABI calibration scan: 2000-2005 UTC - No ABI products generated or distributed
^M ABI Continuous Full Disk Mode (mode 4): 2005-2010 UTC
^M ABI 10-minute Flex Mode (mode 6) resumes: 2010 UTC
^M M-B
^M Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880
^M M-B
^M Web Site(s) for applicable information:
^M See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.
^M
^M This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request^M
^M
^M