^M ^M ^M ^M ^M
^M
Topic: NDE Planned System Upgrade^M

^M

^M

Date/Time Issued: January 30, M-B2019, 2101 UTC

^M

^M

^M

Product(s) or Data Impacted: M-BAll NDE products

^M

^M

^M

Date/Time of Initial Impact: M-BJanuary 31, M-B2019, 1440 UTC

^M

^M

^M

Date/Time of Expected End: January 31, M-B2019, 1710 UTC

^M

^M

^M

Length of Outage: M-BM-B2.5 hrs

^M

^M

^M

Details/Specifics of Change:

^M

Install NDE release 2.0.14

^M
^M

The installation is planned to be done during back orbits. NDE will not be ingesting, processing or distributing data during installation.M-B No data loss expected, but there will be a possible backlog of processing when installation is complete.

^M
^M

Algorithm changes are as follows:

^M
^M

The update extends MiRS's capability to provide ATMS Snowfall Rate (SFR) product from S-NPP. Although there is no change to the PDA short name, the revision number in the MiRS IMG and SND files are changed from v11r1 to v11r3 as shown below.

^M
^M

Current OPS granule files:

^M

NPR-MIRS-IMG_v11r1_snpp_*

^M

NPR-MIRS-SND_v11r1_snpp_*

^M
^M

After the Jan 31 transition:

^M

NPR-MIRS-IMG_v11r3_snpp_*

^M

NPR-MIRS-SND_v11r3_snpp_*

^M
^M

There is no change to the MiRS 33min filename, which doesn't contain revision number.

^M
^M

NPR-MIRS-IMG_33min_v11_snpp_*

^M

NPR-MIRS-SND_33min_v11_snpp_*

^M
^M

Upgrade NDE enterprise cloud, aerosol and cryosphere products from v1.2 to v2.0 (Product shortname starts with "JPSSRR_"). The only NOAA-20 product from this suite for this release is Aerosol Optical Depth (NetCDF and BUFR). The rest of NOAA-20 products will be included in the next release. After upgrade, product shortname in PDA stays the same, but version number in filename will change from v1r2 to v2r0.

^M
^M

Update current operational vegetation products from 4 km to 1km including TCI, TCI and VHI. This version will have capacity to produce the products in GeoTIFF format.

^M
^M

Patch to put the proper satellite identifier in the NOAA-20 ACSPO BUFR data

^M
^M

Due to the upgrade of BUFR toolkit, the SNPP VPW BUFR filename convention is slightly different. Note that the "version" on filename convention is changed from 'v1r0' to 'v2.1'.

^M

PAMV_v1r0_npp_s{15}_e{15}_c{15}.bufr

^M

To

^M

PAMV_v2.1_npp_s{15}_e{15}_c{15}.bufr

^M
^M

Contact Information: M-BFor information on the status of this work, please contact ESPC Operations at ESPCOperations@noaa.gov and 301-817-3880

^M

^M

^M

This message was sent to ESPC.Notification@noaa.gov.M-B You have been sent this and other notifications because you have opted in to receive it.M-B If you wish to unsubscribe please contact the ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880.M-B Please note: it may take up to two business days to process your unsubscribe request.

^M

^M
^M
^M
^M
^M
M-B
^M
^M
^M
^M
^M
^M
^M
^M
^M