Topic: GOES-16 and GOES-17 M-BABI mode 6 testing

Date/Time Issued: February 12, 2019 1452 UTC

Product(s) or Data Impacted: GOES-16 and GOES-17 ABI data

Date/Time of Initial Impact: February 19, 2019 1500 UTC

Date/Time of Expected End: February 22, 2019 1500 UTC

Length of Event: 3 days (72 hours)

M-B

Details/Specifics of Change:

In preparation for eventual transition to mode 6 operations, the GOES-16 and GOES-17 ABI will execute 72 hours of mode 6 operations from 1500 UTC on February 19, 2019 until 1500 UTC on February 22, 2019. Mode 6 operations is a Full Disk every 10 minutes, CONUS every 5 minutes, and 2 meso domains every minute (or 1 domain every 30 seconds). Users may request GOES-16 and GOES-17 MESO coordinate changes as desired, however, users shall not request Flex Mode (mode 3) or Continuous Full Disk Mode (Mode 4) for GOES-16 nor GOES-17 during this test period.

GOES-16 and GOES-17 ABI will both return to Flex Mode (mode 3) at 1500 UTC on February 22, 2019.

If NWS Regions have any operational concerns, please contact the NCEP SDM (301) 683-1500.

Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880

M-B

Web Site(s) for applicable information:

See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.

This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.