Topic: GOES-17 ABI desert monitoring calibration scan
Date/Time Issued: December 6, 2019 1448Z
Product(s) or Data Impacted: GOES-17 ABI outage and mode change
Date/Time of Initial Impact: December 12, 2019 2000Z
Date/Time of Expected End: December 12, 2019 2010Z
Length of Outage: Approximate 5 minute outage followed by 5 minutes of Continuous Full Disk mode
Details/Specifics of Change: A GOES-17 ABI routine desert monitoring calibration scan will occur from 2000-2010Z on December 12, 2019 following the schedule below:
ABI calibration scan: 2000-2005 UTC - No ABI products generated or distributed
ABI Continuous Full Disk Mode (mode 4): 2005-2010Z
ABI 10-minute Flex Mode (mode 6) resumes: 2010Z
Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880
Web Site(s) for applicable information:
See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.
This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request