Topic: GOES-17 ABI mode 6 operations

Date/Time Issued: February 21, 2019 1928 UTC

Product(s) or Data Impacted: GOES-17 ABI data

Date/Time of Initial Impact: February 25, 2019 1400 UTC

Date/Time of Expected End: February 27, 2019 2200 UTC

Length of Event: 56 hours

M-B

Details/Specifics of Change:

GOES-17 ABI will execute 56 hours of mode 6 operations from 25 February 1400 UTC until 27 February 2200 UTC. Users shall not request Flex Mode (mode 3) or Continuous Full Disk Mode (mode 4) for GOES-17 during this period. Mode 6 operations is a Full Disk every 10 minutes, CONUS every 5 minutes, and 2 meso domains every minute (or 1 domain every 30 seconds). Users may request GEOES-17 MESO domain changes as desired.

GOES-17 will return to Flex Mode (mode 3) on 27 February at 2200 UTC.

If NWS Regions have any operational concerns, please contact the NCEP SDM (301) 683-1500.

Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880

M-B

Web Site(s) for applicable information:

See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.

This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.M-BM-B