^M ^M ^M ^M
^M
^M
^M
^M

G16 ABI Desert Monitoring 9/22

^M

^M

^M Topic: GOES-16 ABI desert monitoring calibration scan ^M Date/Time Issued:M-BSeptember 19, 2019 1540Z^M Product(s) or Data Impacted: GOES-16 ABI outage and mode change^M Date/Time of Initial Impact:M-BSeptember 22,M-B2019 M-B1600Z^M Date/Time of Expected End: September 22, 2019 1610Z^M Length of Outage: Approximate 5 minute outage followed by 5 minutes of Continuous Full Disk mode^M Details/Specifics of Change:^M A GOES-16 ABI routine desert monitoring calibration scan will occur from 1600-1610 UTC on September 22, 2019 following the schedule below: M-B^M M-B^M ABI calibration scan: 1600-1605 UTC - no ABI products generated or distributed^M ABI Continuous Full Disk Mode (mode 4): 1605-1610 UTC^M ABI 10-minute Flex Mode (mode 6) resumes: 1610 UTC^M M-B^M Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880^M M-B^M Web Site(s) for applicable information:^M See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.^M
^M

This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request^M

^M
^M
^M
^M
^M
^M
^M
^M