^M ^M ^M ^M ^M
^M

^M Topic: GOES-17 ABI solar calibration scan

^M Date/Time Issued: AprilM-B29, 2019 1716Z^M Product(s) or Data Impacted: GOES-17 ABI product outage^M Date/Time of Initial Impact:M-BMay 5, 2019 1500Z^M Date/Time of Expected End: May 5, 2019 1510Z^M Length of Outage: Approximately 5 minutes at the end of a period of Continuous Full Disk operations^M Details/Specifics of Change:^M On May 5, 2019, GOES-17 ABI 10-minute Flex Mode (mode 6) will be replaced with 10 minutes of Continuous Full Disk (mode 4) from 1500-1510Z. A GOES-17 ABI solar calibration scan will be performed between 1505-1510Z, resulting in an outage of all ABI products. ABI 10-minutes Flex Mode (mode 6) will resume at 1510Z. The next Full Disk scan will populate at 1510Z.^M
^M Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880^M
^M Web Site(s) for applicable information:^M See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.^M
^M This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.
^M
^M ^M
^M
^M