Topic: GOES-17 ABI solar calibration scan scheduled for January 7, 2019

Date/Time Issued: January 11, 2018 1356 UTC

Product(s) or Data Impacted: GOES-17 ABI product outage

Date/Time of Initial Impact: January 13, 2019 0315 UTC

Date/Time of Expected End: January 13, 2019 0330 UTC

Length of Outage: Approximately 10 minutes at the beginning of a period of Continuous Full Disk operations

Details/Specifics of Change:

On January 13, 2019, GOES-17 ABI Flex Mode (mode 3) will be replaced with 15 minutes of Continuous Full Disk (mode 4) from 0315-0330 UTC. A GOES-17 ABI solar calibration scan will be performed between 0315-0325 UTC, resulting in an outage of all ABI products. ABI Flex Mode (mode 3) will resume at 0330 UTC. The next Full Disk scan will populate at 0330 UTC.

Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880

Web Site(s) for applicable information:

See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.

This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.M-BM-B