Topic: GOES-17 ABI solar calibration scan

Date/Time Issued: June 23, 2020 1320z

Product(s) or Data Impacted: GOES-17 ABI product outage

Date/Time of Initial Impact: June 29, 2020 1510 UTC

Date/Time of Expected End: June 29, 2020 1520 UTC

Length of Outage: Approximately 5 minutes at the end of a period of Continuous Full Disk operations

Details/Specifics of Change:

On June 29, 2020, GOES-17 ABI 10-minute Flex Mode (mode 6) will be replaced with 10 minutes of Continuous Full Disk (mode 4) from 1510-1520 UTC. A GOES-17 ABI solar calibration scan will be performed between 1510-1520 UTC, resulting in an outage of all ABI products. ABI 10-minutes Flex Mode (mode 6) will resume at 1520 UTC. The next Full Disk scan will populate at 1520 UTC.

Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880

Web Site(s) for applicable information:

See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.

This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.