Topic: GOES-17 ABI desert monitoring calibration scan

Date/Time Issued: January 23,2020 1653Z

Product(s) or Data Impacted: GOES-17 ABI outage and mode change

Date/Time of Initial Impact:M-B January 29, 2020M-BM-BM-B2000Z

Date/Time of Expected End: January 29,M-B2020 M-B2010Z

Length of Outage: Approximate 5 minute outage followed by 5 minutes of Continuous Full Disk mode

Details/Specifics of Change:

A GOES-17 ABI routine desert monitoring calibration scan will occur from 2000-2010Z on January 29, 2020 following the schedule below: M-B

M-B

ABI calibration scan: 2000-2005 UTC - No ABI products generated or distributed

ABI Continuous Full Disk Mode (mode 4): 2005-2010Z

ABI 10-minute Flex Mode (mode 6) resumes: 2010Z

M-B

Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880

M-B

Web Site(s) for applicable information:

See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.

This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request