Update #2: Observation time of outage is now correctly updated. The CrIS Scene Selection Module went into safe mode at 11:40:40z. That portion of the CrIS instrument was power-cycled and recovered to preface the recovery time at 15:00:26.
Update #1: NPP Satcon returned CrIS sensor to normal operations during rev 46652. All missing CrIS data is unrecoverable.

Topic: NPP CRIS Safe mode

Date/Time Issued: October 28, 2020 1857Z

Product(s) or Data Impacted: All CRIS NPP products

Date/Time of Initial Impact: October 28, 2020 11:40Z
Date/Time of Expected End: October 28, 2020 14:56Z
Length of Outage: 3 hours 16 mins
Details/Specifics of problem: During NPP SVL contact 46651 CRIS went into safehold mode, all CRIS data will be missing and non-recoverable until further notice. Engineering has been notified with a possible fix action TBD.

Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov and 301-817-3880
Web Site(s) for applicable information: N/A
This message was sent by ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive
it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note:
it may take up to two business days to process your unsubscribe request.