Topic: GOES-16 ABI solar calibration scan

Date/Time Issued: March 13, 2020 1452 UTC

Product(s) or Data Impacted: GOES-16 ABI product outage

Date/Time of Initial Impact: March 21, 2020 1100 UTC

Date/Time of Expected End: March 21, 2020 1110 UTC Length of Outage: Approximately 5 minutes at the end of a period of Continuous Full Disk operations

Details/Specifics of Change:

On March 21, 2020, GOES-16 ABI 10-minute Flex Mode (mode 6) will be replaced with 10 minutes of Continuous Full Disk (mode 4) from 1100-1110 UTC. A GOES-16 ABI solar calibration scan will be performed between 1105-1110 UTC, resulting in an outage of all ABI products. ABI 10-minutes Flex Mode (mode 6) will resume at 1110 UTC. The next Full Disk scan will populate at 1110 UTC.

Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880

Web Site(s) for applicable information:

See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.

This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.