Topic: GOES-16 ABI solar calibration scan
Date/Time Issued: May 18, 2022 1410Z
Product(s) or Data Impacted: GOES-16 ABI product outage
Date/Time of Initial Impact: May 25, 2022 1050Z
Date/Time of Expected End: May 25, 2022 1100 Z
Length of Outage: Approximately 5 minutes at the end of a period of Continuous Full Disk operations
Details/Specifics of Change: On May 25, 2022, GOES-16 ABI 10-minute Flex Mode (mode 6) will be replaced with 10 minutes of Continuous Full Disk (mode 4) from 1050-1100 UTC. A GOES-16 ABI solar calibration scan will be performed between 1055-1100 UTC, resulting in an outage of all ABI products. ABI 10-minutes Flex Mode (mode 6) will resume at 1100 UTC. The next Full Disk scan will populate at 1100 UTC.
Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880
Web Site(s) for applicable information:
See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.
This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.