Update #1: Mission notice closed action taken to correct issue. G17 ABI Channel 11 BDS Update. Changing detector 310 from col 5 to 1.
Topic: Degradation (striping) on GOES-17 ABI Band 11 images
Date/Time Issued: August 03, 2022 2020Z
Product or Data Impacted: GOES-17 ABI L1b Band 11 and derived products All Scenes delivered to AWIPS, GRB, PDA.
Date/Time of Initial Impact: July 21, 2022 2200Z
Date/Time of Expected End: August 03, 2022 1945Z
Length of the Outage/Event: 309 Hours and 45 minutes
Details/Specifics of Change: GOES-17 ABI L1b Band 11 and derived products All Scenes delivered to AWIPS, GRB, PDA. GOES-17 has a bad detector on Band 11. The effect is that striping will get worse after 1900z each day and clear at 0900z the next day. A BDS to correct the problem will be forthcoming when it's approved.
Contact information for further information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880 24x7 or goes-r.product.engineering.group@noaa.gov during normal business hours
Web Site(s) for Applicable Information: N/A
This message was sent by ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.