Topic: GOES-16 ABI desert monitoring calibration scan
Date/Time Issued: May 18, 2022 1416Z
Product(s) or Data Impacted: GOES-16 ABI outage and mode change
Date/Time of Initial Impact: May 25, 2022 1600Z
Date/Time of Expected End: May 25, 2022 1610Z
Length of Outage: Approximate 5 minute outage followed by 5 minutes of Continuous Full Disk mode
Details/Specifics of Change: A GOES-16 ABI routine desert monitoring calibration scan will occur from 1600-1610 UTC on May 25, 2022 following the schedule below:
ABI calibration scan: 1600-1605 UTC - no ABI products generated or distributed
ABI Continuous Full Disk Mode (mode 4): 1605-1610Z
ABI 10-minute Flex Mode (mode 6) resumes: 1610Z
Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880
Web Site(s) for applicable information: See https://www.ospo.noaa.gov/Operations/messages.html for this and other satellite related messages.
This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request
--