Update #3: As of 08:35 UTC Oct 29, 2022 (DOY 302), The NOAA-15 AVHRR Scan Motor current has returned to nominal operational ranges ~210 mA. Data quality and Lib products are now at operational status. Instrument and Data Quality Engineering will continue to closely monitor the AVHRR scan motor as well as the relevant L1b data product. This completes the NOAA-15 AVHRR instrument anomaly recovery.
Update #2: As of Oct 27, 2022 (DOY 300), The Scan Motor current continues to trend downwards, currently at ~260 mA. Data quality has improved, and is consistently above 90% per orbit; however, it is still quite a challenge for data applications since there are scattered gaps. Instrument and Data Quality Engineering will continue to closely monitor the AVHRR scan motor as well as the relevant L1b data product.
Update #1: Beginning ~08:00 UTC Oct 24, 2022 (DOY 297), the NOAA-15 AVHRR motor current began to trend downwards from ~302 mA, gradually dropping to ~265 mA as of Oct 26. The scan motor appears to have never fully stalled, with the average current value never reaching the stall value of 302 mA, though the max value did reach that value on a momentary basis repeatedly. Data produced is still degraded, though less so than before. This seems to indicate the scan motor may be grinding through debris and a full stall is no longer imminent, but still possible.
Topic: NOAA-15 AVHRR Motor Current Increase Event
Date/Time Issued: October 29, 2022 1614Z
Product(s) or Data Impacted: AVHRR Products
Date/Time of Initial Impact: Oct 18, 2022 18:00Z
Impacts on Users and Significance: AVHRR products are affected.
Date/Time of Expected End: Unknown
Length of Outage: Ongoing
Details/Specifics of Change: The NOAA-15 AVHRR Scan Motor current began showing signs of instability on Oct 18 at approximately 18:00 UTC, when the current began to gradually rise from about 205 mA to about 250 mA, where it remained until Oct 24. At about 00:00 UTC on Oct 24, the current beganrising again throughout the day, peaking at about 302mA on Oct 25. Scan motor temperature began rising about the same time and is currently steady at ~29°C. The instrument is still producing data, but it is highly degraded. This behavior may be a sign of an impending scan motor stall, but requires further investigation. Options for recovery are limited.
Contact Information for Further Information: ESPC Operations at ESPCOperations@noaa.gov at 301-817-3880 and/or other contacts as necessary
Web Site(s) for applicable information: N/A
This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it make take up to two business days to process your unsubscribe request.