Update #7: Intermittent degradation of GOES-16 data has been resolved.
Update #6: The last observed degraded GOES-16 ABI image, consistent with the degradation that started on 1 December 2022 at 2312Z, occurred at 2100Z (Band 02 Meso-2). The GOES-16 intermittent degradation anomaly was resolved. As of 7 December 2022 at 2101Z all GOES-16 ABI data is nominal. The total length of this data anomaly was 5 days 21 hours and 49 minutes.
Update #5: Intermittent degradation of GOES-16 ABI Band 02 products continues. This intermittent degradation is also occurring in all other GOES-16 ABI bands (L1b, L2 & derived). The investigation of this GOES-16 data anomaly continues.
Update #4: Intermittent degradation of GOES-16 ABI Band 02 products continues. This intermittent degradation is also occurring in all other GOES-16 ABI bands (L1b, L2 & derived). The investigation of this GOES-16 data anomaly continues.
Update #3: Intermittent degradation continues Investigation on-going
Update #2: Intermittent degradation continues Investigation on-going.
Update #1: Intermittent Band 02 degradation continues to be seen: less often than when initially reported, but still at least every 3 hours.
Topic: GOES-16 ABI L1b Band 02, Sectorized Cloud and Moisture Band 02 and derived products delivered to AWIPS, GRB, PDA
Date/Time Issued: December 08, 2022 1456Z
Product or Data Impacted: GOES-16 ABI L1b Band 02, Sectorized Cloud and Moisture Band 02 and derived products All Scenes delivered to AWIPS, GRB, PDA.
Date/Time of Initial Impact: December 01, 2022 2312Z
Date/Time of Expected End: TBD
Length of the Outage/Event: TBD
Details/Specifics of Change: GOES-16 ABI L1b Band 02, Sectorized Cloud and Moisture Band 02 and derived products All Scenes delivered to AWIPS, GRB, PDA. Intermittent degradation to Band 02 images.
contact information for further information: ESPC Operations at ESPCOperations@noaa.gov or 301-817-3880 24x7 or goes-r.product.engineering.group@noaa.gov during normal business hours