Brooks McCall Vessel Activities – July 7, 2010

1. Brooks McCall

2. Sampling roughly 2 km from well head

3. No acoustical equipment

4. Monitoring Techniques include:

* CTD cast (temperature, conductivity, dissolved oxygen, fluorometry)
* Water sampling (VOA and TPH)
* LISST and FluoroFix
* Rototox analysis

5. Chief scientist reported weak evidence of plume well below a thousand meters at the three sites today. Sites tended to be east of the well head.

6. No additional comments.