Topic: NOAA-20 (JPSS-1) Key Performance Parameter (KPP) Data Release/Activation on PDA

M-B

Date/Time Issued: April 2, 2018M-B 1425 UTC

M-B

Product(s) or Data Impacted: NOAA-20 (JPSS-1)M-BKey Performance Parameters (KPPs)

M-B

Date/Time of Initial Impact: April 2, 2018 at 1500 UTC

M-B

Date/Time of Expected End: M-BN/A

M-B

Length of Event: M-BN/A

M-B

Details/Specifics of Change: NESDIS will activate the NOAA-20 KPP data sets on the Product Distribution and Access (PDA) system onM-B April 2, 2018 M-Bstarting at 1500 UTC. KPPM-bM-^@M-^Ys are those NOAA-20 products that have reached provisional/operational status listed below. M-BPDA users subscribed to the SNPP versions of these products should verify that a specified satellite is selected within your respective PDA subscription; otherwise, you will begin to see the NOAA-20 versions of the products arrive at your interface once those aforementioned products are activated.M-BM-B

M-B

The list of NOAA-20 provisional/operational products are:

M-B

CRIS-SCIENCE-RDR
CrIS-FS-SDR
CrIS-SDR
CrIS-SDR-GEO
CrIS_C0431_BUFR
CrIS_C2211_BUFR
ATMS-SCIENCE-RDR
ATMS-SDR
ATMS-SDR-GEO
ATMS-TDR
ATMS_BUFR

VIIRS_I1_IMG_EDR_TIPA01_KNES

VIIRS_I3_IMG_EDR_TIPA03_KNES
VIIRS_I4_IMG_EDR_TIPA04_KNES
VIIRS_I5_IMG_EDR_TIPA05_KNES
VIIRS_M14_EDR_TIPA24_KNES
VIIRS_M15_EDR_TIPA25_KNES
VIIRS_M16_EDR_TIPA26_KNES
VIIRS_NCC_EDR_TIPA10_KNES
VIIRS-SCIENCE-RDR
VIIRS-DNB-GEO
VIIRS-DNB-SDR
VIIRS-I1-SDR
VIIRS-I2-SDR
VIIRS-I3-SDR
VIIRS-I4-SDR
VIIRS-I5-SDR
VIIRS-M1-SDR
VIIRS-IMG-GTM-EDR-GEO
VIIRS-M2-SDR
VIIRS-M3-SDR
VIIRS-M4-SDR
VIIRS-M5-SDR
VIIRS-M6-SDR
VIIRS-M7-SDR
VIIRS-M8-SDR
VIIRS-M9-SDR
VIIRS-M10-SDR
VIIRS-M11-SDR
VIIRS-M12-SDR
VIIRS-M13-SDR
VIIRS-M14-SDR
VIIRS-M15-SDR
VIIRS-M16-SDR
VIIRS-MOD-GEO
VIIRS-MOD-GEO-TC
VIIRS-IMG-GEO
VIIRS-IMG-GEO-TC
VIIRS-I1-IMG-EDR
VIIRS-I2-IMG-EDR
VIIRS-I3-IMG-EDR
VIIRS-I4-IMG-EDR
VIIRS-I5-IMG-EDR
VIIRS-M1ST-EDR
VIIRS-M2ND-EDR
VIIRS-M3RD-EDR
VIIRS-M4TH-EDR
VIIRS-M5TH-EDR
VIIRS-M6TH-EDR
VIIRS-MOD-GTM-EDR-GEO
VIIRS-NCC-EDR
VIIRS-NCC-EDR-GEO

The Beta, Provisional and Full Validation Readiness definitions are:

M-BM-7M-BM-B Beta -

oM-B Product is minimally validated, and may still contain significant identified and unidentified errors.

oM-B Information/data from validation efforts can be used to make initial qualitative or very limited quantitative assessments regarding product fitness-for-purpose.

oM-B Documentation of product performance and identified product performance anomalies, including recommended remediation strategies, exists.

M-BM-7M-BM-B Provisional

oM-B Product performance has been demonstrated through analysis of a large, but still limited (i.e., not necessarily globally or seasonally representative) number of independent measurements obtained from selected locations, time periods, or field campaign efforts.

oM-B Product analyses are sufficient for qualitative, and limited quantitative, determination of product fitness-for-purpose.

oM-B Documentation of product performance, testing involving product fixes, identified product performance anomalies, including recommended remediation strategies, exists.

oM-B Product is recommended for potential operational use (user decision) and in scientific publications after consulting product status documents.

M-BM-7M-BM-B Full Validation

oM-B Product performance has been demonstrated over a large and wide range of representative conditions (i.e., global, seasonal).

oM-B Comprehensive documentation of product performance exists that includes all known product anomalies and their recommended remediation strategies for a full range of retrieval conditions and severity level.

oM-B Product analyses are sufficient for full qualitative and quantitative determination of product fitness-for-purpose.

oM-B Product is ready for operational use based on documented validation findings and user feedback.

oM-B Product validation, quality assurance, and algorithm stewardship continue through the lifetime of the instrument.

M-B

Contact Information for Further Information:M-B SPSD User ServicesM-B spsd.userservices@noaa.gov

M-B

Web Site(s) for applicable information:

Additional details about the data quality can be found here:M-B https://www.star.nesdis.noaa.gov/jpss/AlgorithmMaturity.php

M-B

This message was sent fromM-B ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk atM-B ESPCOperations@noaa.gov M-BorM-B(301) 817-4799. Please note: it may take up to two business days to process your unsubscribe request.