Topic: Weekly Operations Schedule - Week 51

Date/Time Issued: December 13, 2018 1610Z

Product(s) or Data Impacted: See list below.
Date/Time of Initial Impact: December 13, 2018 15:53:47 (from the Eumetsat Weekly Operations Schedule message)
Date/Time of Expected End: See table in detail for on and off switch time
Length of Outage: N/A
Details/Specifics of Change:

Message number: | 5353
Message creation: | Thu Dec 13 15:53:47 GMT+00:00 2018

Type: | Planned Maintenance
Ann Nr: | 3867
Rev: | 5
Start Time: | 2018-06-04 19:02:00.0
End Time: | 2019-02-03 23:59:00.0
Satellites: | Metop-A
Subsystem: | ASCAT
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | ASCAT Extensive Maintenance. Short outages of the ASCAT GDS Level 1, soil moisture and global and regional winds products can be expected, during satellite passes over Turkey during the mentioned period.[Rev2]: Updated End time and date. [Rev3]: End date updated.[Rev4]: End date updated. [Rev5] End date updated.
Status: | scheduled
Issue Time: | 2018-12-05 16:12:38.0
Services: | ASCAT Level 1 - Metop-A ASCAT Soil Moisture - Metop-A EARS-ASCAT ASCAT AHRPT Metop-A OSI SAF - Products

Type: | Service Enhancement
Ann Nr: | 4317
Rev: | 1
Start Time: | 2018-12-17 09:00:00.0
End Time: | 2018-12-17 09:00:00.0
Subject: | product-change
Detail: | Previous versions of four Copernicus Global Land Service products to be discontinued: NDVI, LAI, FAPAR and FCover, in HDF5 format. For full details, see the URL provided below.
Url: | https://www.eumetsat.int/website/home/News/DAT_4146633.html
Status: | scheduled
Issue Time: | 2018-11-21 16:26:31.0
Services: | Copernicus Global Land service

Type: | Service Enhancement
Ann Nr: | 4367
Rev: | 1
Start Time: | 2018-12-17 09:00:00.0
End Time: | 2018-12-17 09:00:00.0
Subject: | new-product
Detail: | New GOES-15 data in netCDF format to be available on EUMETCast Europe. For full details, see the URL provided below.
Url: | https://www.eumetsat.int/website/home/News/DAT_4167864.html
Status: | scheduled
Issue Time: | 2018-12-06 13:52:38.0
Services: | GOES Products

Type: | Planned Maintenance
Ann Nr: | 4375
Rev: | 1
Start Time: | 2018-12-17 12:30:00.0
End Time: | 2018-12-17 13:30:00.0
Subject: | ground-segment-maintenance
Impact: | risk-of-interruption
Detail: | Athens/Kavouri ground station maintenance. Due to this EARS ground segment maintenance there may be disruption to all imager based services.
Status: | scheduled
Issue Time: | 2018-12-12 14:50:22.0
Services: | EARS-ATOVS EARS-AVHRR EARS-ASCAT EARS-IASI EARS-ATMS EARS-CrlS EARS-VIIRS EARS-NWC EARS-VASS

Type: | Planned Maintenance
Ann Nr: | 4379
Rev: | 1
Start Time: | 2018-12-18 08:18:00.0
End Time: | 2018-12-18 08:25:00.0
Satellites: | Metop-B
Subsystem: | SEM
Component: | MEPED
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | SEM MEPED in flight calibration.
Status: | scheduled
Issue Time: | 2018-12-12 15:22:48.0
Services: | SEM L0 - Metop-B SEM AHRPT Metop-B

Type: | Planned Maintenance
Ann Nr: | 4380
Rev: | 1
Start Time: | 2018-12-18 08:18:00.0
End Time: | 2018-12-18 10:01:00.0
Satellites: | Metop-B
Subsystem: | SEM
Component: | TED
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | SEM TED in flight calibration.
Status: | scheduled
Issue Time: | 2018-12-12 15:27:53.0
Services: | SEM L0 - Metop-B SEM AHRPT Metop-B

Type: | Planned Maintenance
Ann Nr: | 4378
Rev: | 1
Start Time: | 2018-12-18 08:53:00.0
End Time: | 2018-12-18 09:00:00.0
Satellites: | Metop-A
Subsystem: | SEM
Component: | MEPED
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | SEM MEPED in flight calibration.
Status: | scheduled
Issue Time: | 2018-12-12 15:22:04.0
Services: | SEM L0 - Metop-A SEM AHRPT Metop-A

Type: | Planned Maintenance
Ann Nr: | 4382
Rev: | 1
Start Time: | 2018-12-18 17:56:00.0
End Time: | 2018-12-18 18:04:00.0
Satellites: | NOAA-20
Subject: | VIIRS Lunar Roll
Impact: | data-unavailable
Detail: | Lunar Calibration.
Status: | scheduled
Issue Time: | 2018-12-12 15:59:16.0
Services: | ATMS Level 1 - JPSS CrIS Level 1 - JPSS VIIRS EDR - JPSS EARS-ATMS EARS-CrlS EARS-VIIRS

Type: | Planned Maintenance
Ann Nr: | 4376
Rev: | 1
Start Time: | 2018-12-18 18:09:00.0
End Time: | 2018-12-18 18:09:00.0
Satellites: | Jason-3
Subject: | in-plane-manoeuvre
Impact: | data-degraded
Detail: | Station keeping manoeuvre. The semi-major axis will be increased by 9.38 m resulting in radial orbit errors in the OGDRs. OGDR products may be degraded 30 minutes before and up to 2 hours after the manoeuvre. This will affect the sea surface height, but not the wind and wave content in the products.
Status: | scheduled
Issue Time: | 2018-12-12 15:15:19.0
Services: | Jason-3 OGDR

Type: | Planned Maintenance
Ann Nr: | 4381
Rev: | 1
Start Time: | 2018-12-18 18:54:00.0
End Time: | 2018-12-18 19:02:00.0
Satellites: | Suomi NPP
Subject: | VIIRS Lunar Roll
Impact: | data-unavailable
Detail: | Lunar Calibration.
Status: | scheduled
Issue Time: | 2018-12-12 15:59:06.0
Services: | ATMS Level 1 - Suomi-NPP VIIRS EDR - Suomi-NPP CrlS Level 1 - Suomi-NPP EARS-ATMS EARS-CrlS EARS-VIIRS Marine Products - Suomi-NPP Atmospheric Products - Suomi-NPP

Type: | Planned Maintenance
Ann Nr: | 4377
Rev: | 1
Start Time: | 2018-12-18 20:08:00.0
End Time: | 2018-12-18 20:08:00.0
Satellites: | Jason-2
Subject: | in-plane-manoeuvre
Impact: | data-degraded
Detail: | Station keeping manoeuvre. The semi-major axis will be increased by 7.94 m resulting in radial orbit errors in the OGDRs. OGDR products may be degraded 30 minutes before and up to 2 hours after the manoeuvre. This will affect the sea surface height, but not the wind and wave content in the products.
Status: | scheduled
Issue Time: | 2018-12-12 15:16:53.0
Services: | Jason-2 OGDR

Type: | Planned Maintenance
Ann Nr: | 4349
Rev: | 2
Start Time: | 2018-12-19 09:21:00.0
End Time: | 2018-12-19 09:55:00.0
Satellites: | Sentinel-3A
Subject: | out-of-plane-manoeuvre
Impact: | data-degraded
Detail: | The exact times will be announced closer to the day of the manoeuvre. [Rev. 2] - Updated Event Start and End times. Reduced data quality for OLCI and SRAL should be expected for data sensed during this period. Reduced data quality for SLSTR can be expected from 09:21 to approximately 11:38
Status: | scheduled
Issue Time: | 2018-12-12 13:02:27.0
Services: | OLCI Level 1 Products - S3A OLCI Level 2 Marine Products - S3A SLSTR Level 1 Products - S3A SLSTR Level 2 Marine Products - S3A SRAL Level 1 Products - S3A SRAL Level 2 Marine Products - S3A

Type: | Planned Maintenance
Ann Nr: | 4383
Rev: | 1
Start Time: | 2018-12-20 08:06:00.0
End Time: | 2018-12-20 08:43:00.0
Satellites: | Sentinel-3B
Subsystem: | SRAL
Subject: | instrument-special-operation
Impact: | data-unavailable
Detail: | SRAL data will be unavailable during this time. OLCI and SLSTR data will be degraded.
Status: | scheduled
Issue Time: | 2018-12-13 13:36:30.0
Services: | SLSTR Level 1 Products - S3B OLCI Level 1 Products - S3B SRAL Level 2 Marine Products - S3B SRAL Level 1 Products - S3B

Type: | Service Enhancement
Ann Nr: | 4366
Rev: | 1
Start Time: | 2019-01-01 07:00:00.0
End Time: | 2019-01-01 07:00:00.0
Subject: | service-change
Detail: | End of the current GOES-15 LRIT data service on EUMETCast Europe and EUMETCast Africa. New GOES-15 data in netCDF format will be available on EUMETCast Europe from 17 December 2018. For more details, see the URL provided below.
Url: | https://www.eumetsat.int/website/home/News/DAT_4167864.html
Status: | scheduled
Issue Time: | 2018-12-06 13:48:28.0
Services: | GOES Products

Type: | Service Enhancement
Ann Nr: | 4335
Rev: | 1
Start Time: | 2019-01-14 09:00:00.0
End Time: | 2019-01-14 09:00:00.0
Subject: | product-change
Detail: | Update to AC SAF IASI SO2 BUFR product. For more details, see the URL provided below.
Url: | https://www.eumetsat.int/website/home/News/DAT_4156656.html
Status: | scheduled
Issue Time: | 2018-11-28 15:11:14.0
Services: | AC SAF - Products

Type: | Planned Maintenance
Ann Nr: | 4270
Rev: | 2
Start Time: | 2019-01-21 09:00:00.0
End Time: | 2019-01-28 09:00:00.0
Satellites: | MET-11
Subject: | instrument-decontamination
Impact: | data-unavailable
Detail: | Instrument decontamination. Meteosat-9 will cover the service during the decontamination period. An outage of up to two repeat cycles can be expected when switching to and from Meteosat-9. For full details, see the URL provided below. [Rev. 2]: Meteosat-9 data will also be disseminated one week before and one week after Meteosat-11 decontamination, i.e. from 14/01 to 04/02/2019. Users wishing to receive the parallel Meteosat data streams should register with our User Helpdesk (ops@eumetsat.int). For full details, see the URL provided below.
Url: | https://www.eumetsat.int/website/home/News/DAT_4127087.html
Status: | scheduled
Issue Time: | 2018-12-13 10:40:41.0
Services: | 0M-0 SEVIRI Level 1.5 Image Data 0M-0 Meteosat Meteorological Products

Name: | EUMETSAT
Address: | Eumetsat-Allee 1 D-64295 Darmstadt Germany
Telephone: | +49 6151 807 3660/3770
Fax: | +49 6151 807 3790
E-mail: | ops@eumetsat.int
Internet: | www.eumetsat.int

You are receiving this email because you are subscribed to our User Notification Service (UNS). You can modify your UNS subscriptions or unsubscribe at any time via our UNS web interface (login to our Earth Observation Portal required).
Any email message from EUMETSAT is sent in good faith but shall neither be binding nor construed as constituting a commitment by EUMETSAT, except where provided for in a written agreement or contract or if explicitly stated in the email. Please note that any views or opinions presented in this email are solely those of the sender and do not necessarily represent those of EUMETSAT. This message and any attachments are intended for the sole use of the addressee(s) and may contain confidential and privileged information. Any unauthorised use, disclosure, dissemination or distribution (in whole or in part) of its contents is not permitted. If you received this message in error, please notify the sender and delete it from your system.