Topic: Weekly Operations Schedule - Week 2

Date/Time Issued: January 03, 2019 1706Z

Product(s) or Data Impacted: See list below.
Date/Time of Initial Impact: January 03, 2019 16:55:34 (from the Eumetsat Weekly Operations Schedule message)
Date/Time of Expected End: See table in detail for on and off switch time
Length of Outage: N/A
Details/Specifics of Change:

Message number: | 5397
Message creation: | Thu Jan 03 16:55:34 GMT+00:00 2019

Type: | Planned Maintenance
Ann Nr: | 3867
Rev: | 5
Start Time: | 2018-06-04 19:02:00.0
End Time: | 2019-02-03 23:59:00.0
Satellites: | Metop-A
Subsystem: | ASCAT
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | ASCAT Extensive Maintenance. Short outages of the ASCAT GDS Level 1, soil moisture and global and regional winds products can be expected, during satellite passes over Turkey during the mentioned period.[Rev2]: Updated End time and date. [Rev3]: End date updated.[Rev4]: End date updated. [Rev5] End date updated.
Status: | scheduled
Issue Time: | 2018-12-05 16:12:38.0
Services: | ASCAT Level 1 - Metop-A ASCAT Soil Moisture - Metop-A EARS-ASCAT ASCAT AHRPT Metop-A OSI SAF - Products

Type: | Planned Maintenance
Ann Nr: | 4360
Rev: | 1
Start Time: | 2018-12-31 00:00:00.0
End Time: | 2019-03-18 00:00:00.0
Satellites: | Metop-A
Subsystem: | GOME-2
Subject: | general-announcement
Impact: | risk-of-degradation
Detail: | The Metop-A satellite with GOME-2 on-board is currently in drifting orbit. As a consequence there are periods during which the GOME-2 instrument will not be able to carry out its daily solar calibration measurement. The second such period will be from 31 December 2018 to 17 March 2019. During this period, the solar mean reference spectrum provided in the Metop-A GOME-2 level-1B product will be automatically replaced by a modelled solar spectrum using information on solar activity from Metop-B. Therefore, it is expected that the quality of both level-1B and level-2 products might undergo slight changes during this period, and there will be an associated risk of degraded product quality for Metop-A GOME-2 products.
Status: | scheduled
Issue Time: | 2018-12-28 09:30:16.0
Services: | GOME-2 Level 1 - Metop-A GOME-2 AHRPT Metop-A AC SAF - Products

Type: | Planned Maintenance
Ann Nr: | 4395
Rev: | 1
Start Time: | 2019-01-06 12:41:00.0
End Time: | 2019-01-06 13:11:00.0
Satellites: | MET-8
Subject: | lunar-eclipse
Impact: | risk-of-degradation
Detail: | Moon eclipse. 12:30 to 13:00 UTC image data may be unavailable or incomplete.
Status: | scheduled
Issue Time: | 2018-12-19 16:43:36.0
Services: | IODC SEVIRI Level 1.5 Image Data IODC Meteosat Meteorological Products

Type: | Planned Maintenance
Ann Nr: | 4411
Rev: | 1
Start Time: | 2019-01-07 05:12:00.0
End Time: | 2019-01-07 09:12:00.0
Satellites: | Metop-A
Subsystem: | IASI
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | External Calibration
Status: | scheduled
Issue Time: | 2019-01-02 15:18:34.0
Services: | IASI Sounding Products - Metop-A IASI Level 1 - Metop-A EARS-IASI IASI AHRPT Metop-A OSI SAF - Products

Type: | Planned Maintenance
Ann Nr: | 4416
Rev: | 1
Start Time: | 2019-01-07 08:00:00.0
End Time: | 2019-01-07 11:00:00.0
Subject: | ground-segment-maintenance
Impact: | risk-of-interruption
Detail: | Update of the EUMETSAT Data Centre Ordering Client. During this time, the Data Centre Ordering Client will not be available and no new orders will be processed. For more details follow the URL below.
Url: | http://www.eumetsat.int/website/home/Data/DataDelivery/EUMETSATDataCentre/OrderingFAQ/index.html?filter=interruptions
Status: | scheduled
Issue Time: | 2019-01-02 15:30:04.0
Services: | EUMETSAT Data Centre

Type: | Service Enhancement
Ann Nr: | 4409
Rev: | 1
Start Time: | 2019-01-07 09:00:00.0
End Time: | 2019-01-07 09:00:00.0
Subject: | general-announcement
Detail: | Indicators for Sentinel-3B OLCI Level 1B, SRAL Level 1B and Level 2 products will be included in the OSSI (Operational Service Status Indicator) available from the EUMETSAT website.
Url: | https://www.eumetsat.int/ossi/
Status: | scheduled
Issue Time: | 2018-12-21 15:12:04.0
Services: |

Type: | Planned Maintenance
Ann Nr: | 4417
Rev: | 1
Start Time: | 2019-01-07 15:02:00.0
End Time: | 2019-01-07 15:08:00.0
Satellites: | Metop-B
Subsystem: | ASCAT
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | Gain Compression
Status: | scheduled
Issue Time: | 2019-01-02 15:31:43.0
Services: | ASCAT Level 1 - Metop-B ASCAT Soil Moisture - Metop-B EARS-ASCAT ASCAT AHRPT Metop-B OSI SAF - Products

Type: | Planned Maintenance
Ann Nr: | 4413
Rev: | 1
Start Time: | 2019-01-08 08:17:00.0
End Time: | 2019-01-08 08:25:00.0
Satellites: | Metop-A
Subsystem: | SEM
Component: | MEPED
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | SEM MEPED in flight calibration.
Status: | scheduled
Issue Time: | 2019-01-02 15:20:59.0
Services: | SEM L0 - Metop-A SEM AHRPT Metop-A

Type: | Planned Maintenance
Ann Nr: | 4410
Rev: | 1
Start Time: | 2019-01-08 09:00:00.0
End Time: | 2019-01-10 09:00:00.0
Satellites: | MET-10
Subject: | monthly-RSS-interruption
Impact: | data-unavailable
Detail: | Monthly interruption. Meteosat-10 Rapid Scanning Service (RSS) will be suspended for scheduled Full Earth Scanning and Ground Segment Maintenance. Meteosat-9 RSS image data, rectified to 9.5 deg E, replaces the Meteosat-10 service. The RSS meteorological product service is not available during this timeframe. An outage of 15 minutes (or slightly more) can be expected when switching to and from Meteosat-9.
Status: | scheduled
Issue Time: | 2019-01-02 15:17:31.0
Services: | RSS SEVIRI Level 1.5 Image Data RSS Meteosat Meteorological Products

Type: | Planned Maintenance
Ann Nr: | 4415
Rev: | 1
Start Time: | 2019-01-08 09:25:00.0
End Time: | 2019-01-08 09:32:00.0
Satellites: | Metop-B
Subsystem: | SEM
Component: | MEPED
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | SEM MEPED in flight calibration.
Status: | scheduled
Issue Time: | 2019-01-02 15:23:31.0
Services: | SEM L0 - Metop-B SEM AHRPT Metop-B

Type: | Planned Maintenance
Ann Nr: | 4412
Rev: | 1
Start Time: | 2019-01-13 18:50:00.0
End Time: | 2019-01-13 19:49:00.0
Satellites: | Metop-A
Subsystem: | GOME-2
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | GOME2 monthly measurements of GOME-2 polarisation (PMD) data in raw readout mode (PMDRAW). The AC SAF Near Real Time Total Column products (Total Column Ozone, the Total Column NO2, and the Tropospheric NO2) will be unavailable.
Status: | scheduled
Issue Time: | 2019-01-02 15:19:33.0
Services: | GOME-2 Level 1 - Metop-A GOME-2 AHRPT Metop-A AC SAF - Products

Type: | Planned Maintenance
Ann Nr: | 4414
Rev: | 1
Start Time: | 2019-01-13 19:44:00.0
End Time: | 2019-01-13 20:43:00.0
Satellites: | Metop-B
Subsystem: | GOME-2
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | GOME2 monthly measurements of GOME-2 polarisation (PMD) data in raw readout mode (PMDRAW). The AC SAF Near Real Time Total Column products (Total Column Ozone, the Total Column NO2, and the Tropospheric NO2) will be unavailable.
Status: | scheduled
Issue Time: | 2019-01-02 15:22:04.0
Services: | GOME-2 Level 1 - Metop-B GOME-2 AHRPT Metop-B AC SAF - Products

Type: | Service Enhancement
Ann Nr: | 4335
Rev: | 1
Start Time: | 2019-01-14 09:00:00.0
End Time: | 2019-01-14 09:00:00.0
Subject: | product-change
Detail: | Update to AC SAF IASI SO2 BUFR product. For more details, see the URL provided below.
Url: | https://www.eumetsat.int/website/home/News/DAT_4156656.html
Status: | scheduled
Issue Time: | 2018-11-28 15:11:14.0
Services: | AC SAF - Products

Type: | Planned Maintenance
Ann Nr: | 4270
Rev: | 2
Start Time: | 2019-01-21 09:00:00.0
End Time: | 2019-01-28 09:00:00.0
Satellites: | MET-11
Subject: | instrument-decontamination
Impact: | data-unavailable
Detail: | Instrument decontamination. Meteosat-9 will cover the service during the decontamination period. An outage of up to two repeat cycles can be expected when switching to and from Meteosat-9. For full details, see the URL provided below. [Rev. 2]: Meteosat-9 data will also be disseminated one week before and one week after Meteosat-11 decontamination, i.e. from 14/01 to 04/02/2019. Users wishing to receive the parallel Meteosat data streams should register with our User Helpdesk (ops@eumetsat.int). For full details, see the URL provided below.
Url: | https://www.eumetsat.int/website/home/News/DAT_4127087.html
Status: | scheduled
Issue Time: | 2018-12-13 10:40:41.0
Services: | 0M-0 SEVIRI Level 1.5 Image Data 0M-0 Meteosat Meteorological Products

Name: | EUMETSAT
Address: | Eumetsat-Allee 1 D-64295 Darmstadt Germany
Telephone: | +49 6151 807 3660/3770
Fax: | +49 6151 807 3790
E-mail: | ops@eumetsat.int
Internet: | www.eumetsat.int

You are receiving this email because you are subscribed to our User Notification Service (UNS). You can modify your UNS subscriptions or unsubscribe at any time via our UNS web interface (login to our Earth Observation Portal required).
Any email message from EUMETSAT is sent in good faith but shall neither be binding nor construed as constituting a commitment by EUMETSAT, except where provided for in a written agreement or contract or if explicitly stated in the email. Please note that any views or opinions presented in this email are solely those of the sender and do not necessarily represent those of EUMETSAT. This message and any attachments are intended for the sole use of the addressee(s) and may contain confidential and privileged information. Any unauthorised use, disclosure, dissemination or distribution (in whole or in part) of its contents is not permitted. If you received this message in error, please notify the sender and delete it from your system.