Topic: NOAA-20 Declared Operational for Environmental Data Records scheduled today at 1530 UTC.

Date/Time Issued: March 7, 2019 1909Z
Product(s) or Data Impacted: NOAA-20 products
Date/Time of Initial Impact: March 7, 2019 1530Z
Date/Time of Expected End: March 7, 2019 1800Z
Length of Outage: 2.5 hours
Details/Specifics of Change:

With installation of NDE release 2.0.15 NOAA-20 EDRs will be operational

The installation is planned to be done during back orbits. NDE will not be ingesting, processing or distributing data during installation. No data loss expected, but there will be a possible backlog of processing when installation is complete.

Algorithm changes are as follows:

NOAA-20 MiRS

This release extends MiRS v11r3 capability to provide NOAA-20 products. All NOAA-20 MiRS products, except snowfall rate (SFR), have passed their provisional maturity review and have been operational. The NOAA-20 SFR is still in Beta, and will become operational sometime after it passes the provisional maturity review.

Although PDA short names remain the same as those of S-NPP, the MiRS IMG and SND files are updated to replace 'snppM-bM-^@M-^\ with "n20" as follows:

NPR-MIRS-IMG_v11r3_n20_* (PDA short name: MIRS_ATMS_IMG)

NPR-MIRS-SND_v11r3_n20_* (PDA short name: MIRS_ATMS_SND)

NPR-MIRS-IMG_33min_v11_n20_* (PDA short name: NPR-MIRS-IMG_33min_v11)

NPR-MIRS-SND_33min_v11_n20_* (PDA short name: NPR-MIRS-SND_33min_v11)

NPR-MIRS-IMG_v11r3_n20_*.tar (PDA shortname: BUNDLED_NUPS_MIRS_ATMS_IMG)

NPR-MIRS-SND_v11r3_n20_*.tar (PDA shortname: BUNDLED_NUPS_MIRS_ATMS_SND)

VIIRS Imagery and Near Constant Contrast GeoTIFF Products

This release includes VIIRS I1, I2, I3, I5 and NCC GeoTIFF products for the J1 satellite & NIC's regions of interest.

NOAA-20 JPSS Risk Reduction Products

This release includes NOAA-20 VIIRS Cloud Mask, Cloud Phase/Type, Cloud Daytime Cloud Properties (DCOMP), Cloud Height (Top and Base), Aerosol Optical Depth and Particle Size, Aerosol Detection, and Volcanic Ash have reached provisional maturity and will be available for public access from PDA. Additionally, NOAA-20 Aerosol Optical Depth will also be available in both BUFR format and NetCDF.

NOAA-20 OMPS V8TOz and V8TOS

This release includes NOAA-20 OMPS V8TOz and V8TOS have passed Provisional Maturity, been declared operational, and will be available for public access from PDA.

NOAA-20 NUCAPS

This release includes NOAA-20 CrIS high resolution of Sensor Data Records (SDR) to include the Cloud Mask and Cloud Height information. In addition, it also includes the NOAA-20 NUCAPS Environmental Data Records (EDR) for Temperature, Water Vapor and Ozone profiles, Outgoing Long Wave Radiations (OLR) as well as trace gases. NUCAPS trace gases include the Carbon Monoxide (CO), Carbon Dioxide (CO2), and Methane (CH4) data products.

Note: To subscribe the AWIPS products from PDA use the following short names that have been changed for the WMO regions IUTN01 M-bM-^@M-^S ITUN09.

NUCAPS_EDR_IUTN11_KNES
NUCAPS_EDR_IUTN12_KNES
NUCAPS_EDR_IUTN13_KNES
NUCAPS_EDR_IUTN14_KNES
NUCAPS_EDR_IUTN15_KNES
NUCAPS_EDR_IUTN16_KNES
NUCAPS_EDR_IUTN17_KNES
NUCAPS_EDR_IUTN18_KNES
NUCAPS_EDR_IUTN19_KNES

VIIRS Polar Winds (VPW)

This release includes NOAA-20 VPW products and updates the version number on operational SNPP VPW products. The NOAA-20 VPW product has passed provisional maturity review and is now declared operational.

1) The file name convention of NOAA-20 VPW products are:

NOAA-20 VPW Products in NetCDF format:

PAMV-VIIRS-CD-NH_v2r1_j01_s*_e*_c*.nc

PAMV-VIIRS-CD-SH_v2r1_j01_s*_e*_c*.nc

Products in BUFR format:

PAMV_v2r1_j01_s*_e*_c*.bufr

2) Similar to NOAA-20 VPW, the file name convention of SNPP VPW products will be updated:

SNPP VPW Products in NetCDF format:

From

PAMV-VIIRS-CD-NH_v2.1_npp_s*_e*_c*.nc

To

PAMV-VIIRS-CD-NH_v2r1_npp_s*_e*_c*.nc

From

PAMV-VIIRS-CD-SH_v2.1_npp_s*_e*_c*.nc

To

PAMV-VIIRS-CD-SH_v2r1_npp_s*_e*_c*.nc

SNPP VPW Products in BUFR format:

From

PAMV_v2.1_npp_s*_e*_c*.bufr

To

PAMV_v2r1_npp_s*_e*_c*.bufr

Contact Information: For information on the status of this work, please contact ESPC Operations at ESPCOperations@noaa.gov and 301-817-3880

Web Site(s) for applicable information: N/A

This message was sent to ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If you wish to unsubscribe please contact the ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.