Topic: Eumetsat Weekly Operations Schedule - Week 05 Issue 6 (Update of Announcement 5522)

Date/Time Issued: January 30, 2020 1709Z

Product(s) or Data Impacted:M-B See list below.

Date/Time of Initial Impact:M-B January 30, 2020 1647ZM-B (from the Eumetsat Weekly Operations Schedule message)

Date/Time of Expected End:M-B See table in detail for on and off switch time M-B

Length of Outage:M-B N/A

Message number: | 6604
Message creation: | Thu Jan 30 16:47:16 GMT+00:00 2020

Type: | Service Enhancement
Ann Nr: | 4920
Rev: | 1
Start Time: | 2019-06-27 09:00:00.0
End Time: | 2019-06-27 09:00:00.0
Subject: | general-announcement
Detail: | There is an issue with the latest EUMETCast software package, affecting Linux operating systems when the Tellicast client software (version 2.14.5) is used in combination with the Safenet drivers. A new alpha version of Tellicast, with a fix of the issue, is available for download. See the URL provided below.
Url: | https://www.eumetsat.int/website/home/News/DAT_4451027.html
Issue Time: | 2019-06-27 11:18:18.0
Services: |

Type: | Planned Maintenance
Ann Nr: | 5355
Rev: | 1
Start Time: | 2019-11-14 00:00:00.0
End Time: | 2020-04-15 00:00:00.0
Satellites: | Metop-A
Subsystem: | GOME-2
Subject: | general-announcement
Impact: | data-degraded
Detail: | The Metop-A satellite with GOME-2 on-board is currently in drifting orbit. As a consequence there are periods during which the GOME-2 instrument is not able to carry out its daily solar calibration measurement. The third such period will be from 14 November 2019 to 14 April 2020. During this period, the solar mean reference spectrum provided in the Metop-A GOME-2 level-1B product will be automatically replaced by a modelled solar spectrum using information on solar activity from Metop-B. Therefore, it is expected that the quality of both level-1B and level-2 products might undergo slight changes during this period, and there will be an associated risk of degraded product quality for Metop-A GOME-2 products.
Status: | scheduled
Issue Time: | 2020-01-10 07:39:08.0
Services: | GOME-2 Level 1 - Metop-A GOME-2 AHRPT Metop-A AC SAF - Products

Type: | Planned Maintenance
Ann Nr: | 5402
Rev: | 2
Start Time: | 2019-12-04 14:00:00.0
End Time: | 2020-02-19 14:00:00.0
Satellites: | Metop-C
Subject: | general-announcement
Impact: | data-degraded
Detail: | Drift to a new orbital position. During this period, Metop-C will not be following the reference orbit, with a drifting ground track and phase with respect to Metop-B. Some instrument products may be degraded. A small impact on the number and quality of AVHRR wind products might be observed during this period. [Rev. 2]: End date updated.
Status: | scheduled
Issue Time: | 2020-01-10 07:39:23.0
Services: | SEM L0 - Metop-C AVHRR Level 1 - Metop-C AMSU-A Level 1 - Metop-C MHS Level 1 - Metop-C Multi-sensor Products - Metop-C IASI Sounding products- Metop-C IASI Level 1 - Metop-C EARS-ATOVS EARS-IASI EARS-AVHRR AMSU-A AHRPT Metop-C A-DCS AHRPT Metop-C AVHRR AHRPT Metop-C HIRS AHRPT Metop-C MHS AHRPT Metop-C IASI AHRPT Metop-C SEM AHRPT Metop-C

Type: | Planned Maintenance
Ann Nr: | 5475
Rev: | 1
Start Time: | 2020-01-06 00:00:00.0
End Time: | 2020-02-17 00:00:00.0
Satellites: | Metop-A
Subsystem: | ASCAT
Subject: | general-announcement
Impact: | risk-of-interruption
Detail: | Calibrations to support transponder test. Outages of products can be expected, during satellite passes over Turkey.
Status: | scheduled
Issue Time: | 2019-12-18 16:16:48.0
Services: | ASCAT Level 1 - Metop-A ASCAT Soil Moisture - Metop-A

Type: | Planned Maintenance
Ann Nr: | 5450
Rev: | 1
Start Time: | 2020-01-06 09:00:00.0
End Time: | 2020-02-03 09:00:00.0
Satellites: | MET-10
Subject: | yearly-RSS-interruption
Impact: | data-unavailable
Detail: | Yearly interruption. Meteosat-10 Rapid Scanning Service (RSS) will be suspended for scheduled Full Earth Scanning and Ground Segment maintenance. During this period, there will be no RSS gap filling by Meteosat-9.
Status: | scheduled
Issue Time: | 2019-12-11 16:39:52.0
Services: | RSS SEVIRI Level 1.5 Image Data RSS Meteosat Meteorological Products

Type: | Planned Maintenance
Ann Nr: | 5449
Rev: | 1
Start Time: | 2020-01-27 09:00:00.0
End Time: | 2020-02-03 09:00:00.0
Satellites: | MET-9
Subject: | instrument-decontamination
Detail: | SEVIRI decontamination. Meteosat-9 will not be available as backup spacecraft for the Full Earth Scan service in the event of Meteosat-11 anomalies. Meteosat-10 will be the backup spacecraft instead. For full details, see the related URL provided below.
Url: | https://www.eumetsat.int/website/home/News/DAT_4762227.html
Status: | scheduled
Issue Time: | 2019-12-11 14:53:03.0
Services: | 0M-BM-0 SEVIRI Level 1.5 Image Data 0M-BM-0 Meteosat Meteorological Products

Type: | Planned Maintenance
Ann Nr: | 5596
Rev: | 1
Start Time: | 2020-01-29 00:00:00.0
End Time: | 2021-12-31 23:59:00.0
Satellites: | Metop-A
Subsystem: | HRPT
Subject: | general-announcement
Impact: | risk-of-degradation
Detail: | HRPT switching zone drift. The Metop-A satellite is currently in drifting orbit. As a consequence the geographical zones, defined to control the switching times of the satelliteM-bM-^@M-^Ys HRPT system, are drifting westwards at a rate of 0.02M-BM-0 per day. Users near the borders of switching zones might experience small changes in their acquisition times of the HRPT signal. On-board timings will be updated approximately every 8 months to compensate for the drift geolocation. A dedicated announcement will be issued in advance of each of these updates.
Status: | scheduled
Issue Time: | 2020-01-30 08:46:22.0
Services: | ASCAT AHRPT Metop-A A-DCS AHRPT Metop-A AMSU-A AHRPT Metop-A AVHRR AHRPT Metop-A GOME-2 AHRPT Metop-A GRAS AHRPT Metop-A HIRS AHRPT Metop-A MHS AHRPT Metop-A SEM AHRPT Metop-A IASI AHRPT Metop-A

Type: | Planned Maintenance
Ann Nr: | 5600
Rev: | 1
Start Time: | 2020-01-30 08:00:00.0
Subject: | ground-segment-maintenance
Impact: | risk-of-interruption
Detail: | Due to system maintenance, the SARAL service is in a risk-state and product degradation or losses can be expected, until further notice. This is affecting all SARAL products distributed on EUMETCast.
Status: | scheduled
Issue Time: | 2020-01-30 16:16:27.0
Services: | SARAL Products

Type: | Service Enhancement
Ann Nr: | 5599
Rev: | 1
Start Time: | 2020-01-30 09:00:00.0
End Time: | 2020-01-30 09:00:00.0
Subject: | general-announcement
Detail: | The reprocessing of all Sentinel-3 SRAL/MWR data to the latest standards is on-going, and the currently reprocessed datasets are now available. For full details, see the URL provided below.
Url: | https://www.eumetsat.int/website/home/News/DAT_4852830.html
Status: | scheduled
Issue Time: | 2020-01-30 10:35:23.0
Services: | SRAL Level 2 Marine Products - S3A SRAL Level 2 Marine Products - S3B

Type: | Service Enhancement
Ann Nr: | 5470
Rev: | 2
Start Time: | 2020-01-31 16:00:00.0
End Time: | 2020-03-02 16:00:00.0
Subject: | service-change
Detail: | NOAA plans to terminate the GOES-15 Imager service on 31 January 2020. The GOES-15 Imager L1b data in netCDF format provided by EUMETSAT will stop being distributed on EUMETCast at the same time. [Rev. 2]: End date updated. NOAA has announced an extension of the GOES-15 imager service to 2 March 2020. The provision by EUMETSAT of GOES-15 L1b data in netCDF will continue until then.
Status: | scheduled
Issue Time: | 2020-01-30 10:17:31.0
Services: | GOES Products

Type: | Planned Maintenance
Ann Nr: | 5580
Rev: | 1
Start Time: | 2020-02-03 09:00:00.0
End Time: | 2020-02-03 17:00:00.0
Subject: | ground-segment-maintenance
Impact: | data-unavailable
Detail: | IASI Level 2 Patch installation V6.5.9 and System upgrade. Correction of two anomalies detected on the IASI L2 V 6.5 which is operational since the 4th December 2019: - Cloud: cloud top temperature values were sometimes incorrectly supplied although no clouds could actually be retrieved. All cloud parameters are now reset to NaN in the absence of a cloud retrieval. - SO2: Information about missing input IASI data were not copied into the SO2 quality flag, which was also preventing the use of forecast data instead of IASI L2 profiles when those were of degraded quality. The correct processing and flagging have been restored. Please note that an outage of up to 8 hours during working hours might be encountered.
Status: | scheduled
Issue Time: | 2020-01-30 16:42:22.0
Services: | IASI Sounding Products - Metop-A IASI Sounding products- Metop-C IASI Sounding Products - Metop-B

Type: | Planned Maintenance
Ann Nr: | 5590
Rev: | 1
Start Time: | 2020-02-03 15:53:00.0
End Time: | 2020-02-03 16:00:00.0
Satellites: | Metop-B
Subsystem: | ASCAT
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | Gain Compression
Status: | scheduled
Issue Time: | 2020-01-29 16:15:13.0
Services: | ASCAT Soil Moisture - Metop-B ASCAT Level 1 - Metop-B EARS-ASCAT ASCAT AHRPT Metop-B OSI SAF - Products

Type: | Planned Maintenance
Ann Nr: | 5581
Rev: | 1
Start Time: | 2020-02-04 06:13:00.0
End Time: | 2020-02-04 06:14:00.0
Satellites: | MET-11
Subject: | in-plane-manoeuvre
Impact: | data-degraded
Detail: | East-West Station Keeping Manoeuvre. Users may experience degraded image quality and degraded meteorological product quality up to a few hours after the manoeuvre.
Status: | scheduled
Issue Time: | 2020-01-29 15:24:24.0
Services: | 0M-BM-0 SEVIRI Level 1.5 Image Data 0M-BM-0 Meteosat Meteorological Products

Type: | Planned Maintenance
Ann Nr: | 5585
Rev: | 1
Start Time: | 2020-02-04 08:01:00.0
End Time: | 2020-02-04 08:08:00.0
Satellites: | Metop-A
Subsystem: | SEM
Component: | MEPED
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | SEM MEPED in flight calibration.
Status: | scheduled
Issue Time: | 2020-01-29 16:10:32.0
Services: | SEM L0 - Metop-A SEM AHRPT Metop-A

Type: | Planned Maintenance
Ann Nr: | 5586
Rev: | 1
Start Time: | 2020-02-04 08:01:00.0
End Time: | 2020-02-04 09:44:00.0
Satellites: | Metop-A
Subsystem: | SEM
Component: | TED
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | SEM TED in flight calibration.
Status: | scheduled
Issue Time: | 2020-01-29 16:11:04.0
Services: | SEM L0 - Metop-A SEM AHRPT Metop-A

Type: | Planned Maintenance
Ann Nr: | 5588
Rev: | 1
Start Time: | 2020-02-04 08:29:00.0
End Time: | 2020-02-04 08:36:00.0
Satellites: | Metop-C
Subsystem: | SEM
Component: | MEPED
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | SEM MEPED in flight calibration.
Status: | scheduled
Issue Time: | 2020-01-29 16:12:34.0
Services: | SEM L0 - Metop-C SEM AHRPT Metop-C

Type: | Planned Maintenance
Ann Nr: | 5595
Rev: | 1
Start Time: | 2020-02-04 09:00:00.0
End Time: | 2020-02-04 10:30:00.0
Subject: | ground-segment-maintenance
Impact: | risk-of-interruption
Detail: | Svalbard station SG-7 Antenna Maintenance. Risk of service interruption for FY, NOAA-20 and SNPP passes. There may be disruption to all Svalbard acquired EARS services during the indicated maintenance period.
Issue Time: | 2020-01-29 16:44:45.0
Services: | EARS-ATOVS EARS-AVHRR EARS-ASCAT EARS-ATMS EARS-IASI EARS-CrlS EARS-NWC EARS-VASS EARS-VIIRS

Type: | Planned Maintenance
Ann Nr: | 5573
Rev: | 1
Start Time: | 2020-02-04 09:00:00.0
End Time: | 2020-02-04 17:00:00.0
Satellites: | Metop-A,Metop-B,Metop-C
Subsystem: | GRAS
Subject: | ground-segment-maintenance
Impact: | risk-of-interruption
Detail: | Software Release of GRAS PPF. Changes to the GRAS Level 1 product algorithms. The algorithm changes include technical improvements and bug fixes, as well as support to the changed data formats of the auxiliary files provided by the Radio Occultation Support Network (RSN). The first deployment will be on 4 February 2020, still using the current RSN auxiliary files. The second deployment will be on 12 February 2020, using the changed RSN auxiliary files. There is a risk of an interruption of GRAS production and a temporary deterioration of product timeliness, between 09:00 and 17:00 UTC.
Status: | scheduled
Issue Time: | 2020-01-23 09:45:00.0
Services: | GRAS Level 1 - Metop-A GRAS Level 1 - Metop-B GRAS Level 1 - Metop-C

Type: | Planned Maintenance
Ann Nr: | 5587
Rev: | 1
Start Time: | 2020-02-04 09:16:00.0
End Time: | 2020-02-04 09:23:00.0
Satellites: | Metop-B
Subsystem: | SEM
Component: | MEPED
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | SEM MEPED in flight calibration.
Status: | scheduled
Issue Time: | 2020-01-29 16:12:02.0
Services: | SEM L0 - Metop-B SEM AHRPT Metop-B

Type: | Planned Maintenance
Ann Nr: | 5589
Rev: | 1
Start Time: | 2020-02-05 05:12:00.0
End Time: | 2020-02-05 09:12:00.0
Satellites: | Metop-B
Subsystem: | IASI
Subject: | instrument-calibration
Impact: | data-unavailable
Detail: | External Calibration
Status: | scheduled
Issue Time: | 2020-01-29 16:13:45.0
Services: | IASI Level 1 - Metop-B IASI Sounding Products - Metop-B EARS-IASI IASI AHRPT Metop-B OSI SAF - Products

Type: | Planned Maintenance
Ann Nr: | 5593
Rev: | 1
Start Time: | 2020-02-05 08:11:00.0
End Time: | 2020-02-05 08:19:00.0
Satellites: | NOAA-20
Subject: | VIIRS Lunar Roll
Impact: | data-unavailable
Detail: | Lunar Calibration.
Status: | scheduled
Issue Time: | 2020-01-30 09:16:08.0
Services: | ATMS Level 1 - JPSS CrIS Level 1 - JPSS VIIRS EDR - JPSS SNPP - JPSS Copernicus data

Type: | Planned Maintenance
Ann Nr: | 5560
Rev: | 2
Start Time: | 2020-02-05 08:32:00.0
End Time: | 2020-02-05 09:07:00.0
Satellites: | Sentinel-3B
Subject: | out-of-plane-manoeuvre
Impact: | data-degraded
Detail: | The exact times will be announced closer to the day of the manoeuvre. [Rev.2] Event Start and End times revised. Reduced data quality for OLCI and SRAL should be expected for data sensed during this period. Reduced data quality for SLSTR can be expected from 08:25 to 10:53
Status: | scheduled
Issue Time: | 2020-01-29 09:35:01.0
Services: | OLCI Level 1 Products - S3B SLSTR Level 2 Marine Products - S3B OLCI Level 2 Marine Products - S3B SLSTR Level 1 Products - S3B SRAL Level 2 Marine Products - S3B SRAL Level 1 Products - S3B

Type: | Service Enhancement
Ann Nr: | 5565
Rev: | 1
Start Time: | 2020-02-05 09:00:00.0
End Time: | 2020-02-05 09:00:00.0
Subject: | service-change
Detail: | More data to be added to the following regional data services: EARS-ATOVS, EARS-IASI, EARS-ATMS and EARS-CrIS. For more details, see the URL provided below.
Url: | https://www.eumetsat.int/website/home/News/DAT_4825058.html
Status: | scheduled
Issue Time: | 2020-01-22 15:04:27.0
Services: | EARS-IASI EARS-ATOVS EARS-CrlS EARS-ATMS

Type: | Planned Maintenance
Ann Nr: | 5592
Rev: | 1
Start Time: | 2020-02-05 09:01:00.0
End Time: | 2020-02-05 09:09:00.0
Satellites: | Suomi NPP
Subject: | VIIRS Lunar Roll
Impact: | data-unavailable
Detail: | Lunar Calibration.
Status: | scheduled
Issue Time: | 2020-01-30 09:15:18.0
Services: | CrIS Level 1 - JPSS VIIRS EDR - JPSS ATMS Level 1 - JPSS EARS-VIIRS SNPP - JPSS Copernicus data

Type: | Planned Maintenance
Ann Nr: | 5522
Rev: | 2
Start Time: | 2020-02-05 12:22:00.0
End Time: | 2020-02-05 12:23:00.0
Satellites: | Metop-C
Subject: | in-plane-manoeuvre
Impact: | data-degraded
Detail: | Routine in-plane manoeuvre. Reduced data quality should be expected for data sensed during this period. The exact burn time will be announced closer to the day of the manoeuvre. [Rev. 2] : Manoeuvre Execution time updated. Burn time: 12:22:00 UTC. Duration: 36.32 seconds.
Status: | scheduled
Issue Time: | 2020-01-29 16:02:44.0
Services: | SEM L0 - Metop-C AVHRR Level 1 - Metop-C AMSU-A Level 1 - Metop-C MHS Level 1 - Metop-C ASCAT Level 1 - Metop-C IASI Level 1 - Metop-C GRAS Level 1 - Metop-C GOME-2 Level 1 - Metop-C A-DCS AHRPT Metop-C AMSU-A AHRPT Metop-C ASCAT AHRPT Metop-C AVHRR AHRPT Metop-C GOME-2 AHRPT Metop-C GRAS AHRPT Metop-C HIRS AHRPT Metop-C IASI AHRPT Metop-C MHS AHRPT Metop-C SEM AHRPT Metop-C

Type: | Planned Maintenance
Ann Nr: | 5582
Rev: | 1
Start Time: | 2020-02-06 08:45:00.0
End Time: | 2020-02-18 09:45:00.0
Satellites: | MET-8
Subject: | Sun-colinearity
Impact: | risk-of-degradation
Detail: | Sun Co-linearity. Repeat cycles 08:45 to 09:45 may be affected.
Status: | scheduled
Issue Time: | 2020-01-29 15:43:52.0
Services: | IODC SEVIRI Level 1.5 Image Data IODC Meteosat Meteorological Products

Type: | Planned Maintenance
Ann Nr: | 5594
Rev: | 1
Start Time: | 2020-02-06 13:00:00.0
End Time: | 2020-02-06 14:00:00.0
Subject: | ground-segment-maintenance
Impact: | risk-of-interruption
Detail: | EUMETView maintenance. Service disruption can be expected during the indicated time period.
Status: | scheduled
Issue Time: | 2020-01-29 16:33:22.0
Services: | Web Service

Type: | Planned Maintenance
Ann Nr: | 5598
Rev: | 1
Start Time: | 2020-02-07 10:37:00.0
End Time: | 2020-02-07 13:59:00.0
Satellites: | Sentinel-3A
Subsystem: | SRAL
Subject: | instrument-special-operation
Impact: | data-unavailable
Detail: | At 10:37 SRAL will be manually commanded to "Stand by" mode for ~2 mins in order to change the TC_NAV source from DORIS to GNSS. Degradation of data can be expected for ~2-4 mins after the activity due to manual commanding of SRAL mode transitions (Open loop <-> Close loop) At 13:57 SRAL will be once again commanded to Stand by" mode for ~2 mins in order to change the TC_NAV source from GNSS back to DORIS. Degradation of data can be expected for ~2-4 mins after the activity due to manual commanding of SRAL mode transitions (Open loop <-> Close loop).
Status: | scheduled
Issue Time: | 2020-01-30 09:49:47.0
Services: | SRAL Level 1 Products - S3A SRAL Level 2 Marine Products - S3A

Type: | Planned Maintenance
Ann Nr: | 5566
Rev: | 1
Start Time: | 2020-02-07 20:30:00.0
End Time: | 2020-03-30 20:30:00.0
Satellites: | MET-8
Subject: | eclipse-season
Impact: | risk-of-degradation
Detail: | There is a risk of degraded image quality every night from 20:30 to 23:00 in the given time period.
Status: | scheduled
Issue Time: | 2020-01-22 16:24:40.0
Services: | IODC SEVIRI Level 1.5 Image Data IODC Meteosat Meteorological Products

Type: | Planned Maintenance
Ann Nr: | 5597
Rev: | 1
Start Time: | 2020-02-09 00:00:00.0
End Time: | 2020-02-11 00:00:00.0
Satellites: | Metop-A
Subsystem: | HRPT
Subject: | general-announcement
Impact: | risk-of-degradation
Detail: | HRPT switching zone update. An update of the Metop-A on-board HRPT switching zones timings will be performed to compensate for the zone drift in geolocation due to spacecraftM-bM-^@M-^Ys own drifting orbit. This will result in a shift in HRPT switching zones by 6M-BM-0 eastward. HRPT users near the borders of switching zones may experience degradation in service availability for Metop-A HRPT.
Status: | scheduled
Issue Time: | 2020-01-30 09:11:47.0
Services: | ASCAT AHRPT Metop-A A-DCS AHRPT Metop-A AMSU-A AHRPT Metop-A AVHRR AHRPT Metop-A GOME-2 AHRPT Metop-A HIRS AHRPT Metop-A IASI AHRPT Metop-A MHS AHRPT Metop-A GRAS AHRPT Metop-A SEM AHRPT Metop-A

Type: | Planned Maintenance
Ann Nr: | 5545
Rev: | 1
Start Time: | 2020-02-12 09:00:00.0
End Time: | 2020-02-12 09:00:00.0
Satellites: | Metop-A
Subject: | in-plane-manoeuvre
Impact: | data-degraded
Detail: | Routine in-plane manoeuvre. Reduced data quality should be expected for data sensed during this period. The exact burn time will be announced closer to the day of the manoeuvre.
Status: | scheduled
Issue Time: | 2020-01-15 15:37:46.0
Services: | SEM L0 - Metop-A AVHRR Level 1 - Metop-A AMSU-A Level 1 - Metop-A HIRS Level 1 - Metop-A MHS Level 1 - Metop-A ASCAT Level 1 - Metop-A IASI Level 1 - Metop-A GRAS Level 1 - Metop-A GOME-2 Level 1 - Metop-A ATOVS Sounding products - Metop-A IASI Sounding Products - Metop-A ASCAT Soil Moisture - Metop-A AVHRR Polar Winds - Metop-A Multi-Sensor Products - Metop-A A-DCS AHRPT Metop-A AMSU-A AHRPT Metop-A ASCAT AHRPT Metop-A AVHRR AHRPT Metop-A GOME-2 AHRPT Metop-A GRAS AHRPT Metop-A HIRS AHRPT Metop-A IASI AHRPT Metop-A MHS AHRPT Metop-A SEM AHRPT Metop-A

Type: | Planned Maintenance
Ann Nr: | 5574
Rev: | 1
Start Time: | 2020-02-12 09:00:00.0
End Time: | 2020-02-12 17:00:00.0
Satellites: | Metop-A,Metop-B,Metop-C
Subsystem: | GRAS
Subject: | ground-segment-maintenance
Impact: | risk-of-interruption
Detail: | Software Release of GRAS PPF. Changes to the GRAS Level 1 product algorithms. The algorithm changes include technical improvements and bug fixes, as well as support to the changed data formats of the auxiliary files provided by the Radio Occultation Support Network (RSN). This message refers to the second phase of the deployment which will use the changed RSN auxiliary files (after a first phase planned to take place on 04 February 2020).
Status: | scheduled
Issue Time: | 2020-01-23 09:37:29.0
Services: | GRAS Level 1 - Metop-A GRAS Level 1 - Metop-C GRAS Level 1 - Metop-B

Type: | Planned Maintenance
Ann Nr: | 5572
Rev: | 1
Start Time: | 2020-02-19 09:00:00.0
End Time: | 2020-02-19 09:00:00.0
Satellites: | Metop-C
Subject: | in-plane-manoeuvre
Detail: | Drift stop manoeuvre. Some instrument data will be unavailable or degraded during this period.The exact burn time and instrument affected outage will be announced closer to the day of the manoeuvre. Reduced data quality should be expected for data sensed during this period.
Status: | scheduled
Issue Time: | 2020-01-29 16:03:40.0
Services: | AVHRR Level 1 - Metop-C AMSU-A Level 1 - Metop-C SEM L0 - Metop-C IASI Sounding products- Metop-C MHS Level 1 - Metop-C Multi-sensor Products - Metop-C IASI Level 1 - Metop-C EARS-ATOVS EARS-AVHRR EARS-IASI A-DCS AHRPT Metop-C AVHRR AHRPT Metop-C AMSU-A AHRPT Metop-C HIRS AHRPT Metop-C IASI AHRPT Metop-C MHS AHRPT Metop-C SEM AHRPT Metop-C

Type: | Planned Maintenance
Ann Nr: | 5567
Rev: | 1
Start Time: | 2020-02-24 22:30:00.0
End Time: | 2020-04-13 01:00:00.0
Satellites: | MET-10
Subject: | eclipse-season
Impact: | risk-of-degradation
Detail: | There is a risk of degraded image quality every night from 22:30 to 01:00 next day in the given time period.
Status: | scheduled
Issue Time: | 2020-01-22 16:27:24.0
Services: | RSS SEVIRI Level 1.5 Image Data RSS Meteosat Meteorological Products

Type: | Planned Maintenance
Ann Nr: | 5583
Rev: | 1
Start Time: | 2020-02-25 11:15:00.0
End Time: | 2020-03-07 12:15:00.0
Satellites: | MET-10
Subject: | Sun-colinearity
Impact: | risk-of-interruption
Detail: | Sun Co-linearity. Repeat cycles 11:15 to 12:15 may be affected.
Status: | scheduled
Issue Time: | 2020-01-29 15:48:45.0
Services: | RSS Meteosat Meteorological Products RSS SEVIRI Level 1.5 Image Data

Type: | Planned Maintenance
Ann Nr: | 5591
Rev: | 1
Start Time: | 2020-02-26 09:00:00.0
End Time: | 2020-03-02 09:00:00.0
Satellites: | Metop-C
Subsystem: | IASI
Subject: | instrument-decontamination
Impact: | data-unavailable
Detail: | IASI Decontamination.
Status: | scheduled
Issue Time: | 2020-01-29 16:18:53.0
Services: | IASI Sounding products- Metop-C IASI Level 1 - Metop-C EARS-IASI IASI AHRPT Metop-C OSI SAF - Products

Type: | Planned Maintenance
Ann Nr: | 5568
Rev: | 1
Start Time: | 2020-02-27 23:00:00.0
End Time: | 2020-04-12 01:30:00.0
Satellites: | MET-11
Subject: | eclipse-season
Impact: | risk-of-degradation
Detail: | There is a risk of degraded image quality every night from 23:00 to 01:30 next day in the given time period
Status: | scheduled
Issue Time: | 2020-01-22 16:29:43.0
Services: | 0M-BM-0 SEVIRI Level 1.5 Image Data 0M-BM-0 Meteosat Meteorological Products

Type: | Planned Maintenance
Ann Nr: | 5584
Rev: | 1
Start Time: | 2020-02-28 12:00:00.0
End Time: | 2020-03-09 13:00:00.0
Satellites: | MET-11
Subject: | Sun-colinearity
Impact: | risk-of-degradation
Detail: | Sun Co-linearity. Repeat cycles 12:00 to 13:00 may be affected.
Status: | scheduled
Issue Time: | 2020-01-29 15:51:07.0
Services: | 0M-BM-0 SEVIRI Level 1.5 Image Data 0M-BM-0 Meteosat Meteorological Products

Type: | Service Enhancement
Ann Nr: | 5421
Rev: | 1
Start Time: | 2020-03-02 09:00:00.0
End Time: | 2020-03-02 09:00:00.0
Subject: | general-announcement
Detail: | The NOAA Direct Broadcast Real-Time Network (DBRTN) data, currently distributed on EUMETCast, will be removed on 2 March 2020. For full details, see the URL provided below.
Url: | https://www.eumetsat.int/website/home/News/DAT_4759427.html
Status: | scheduled
Issue Time: | 2019-12-04 11:30:54.0
Services: | NDB (NOAA Direct Broadcast)

Type: | Service Enhancement
Ann Nr: | 5159
Rev: | 1
Start Time: | 2020-06-01 09:00:00.0
End Time: | 2020-06-01 09:00:00.0
Subject: | product-change
Detail: | A new BUFR encoding sequence will be introduced in June 2020 for all EUMETSATM-bM-^@M-^Ys wind products. For full details and sample files, see the URL provided below.
Url: | http://www.eumetsat.int/website/home/News/DAT_4593260.html
Status: | scheduled
Issue Time: | 2019-09-11 16:22:14.0
Services: | 0M-BM-0 Meteosat Meteorological Products RSS Meteosat Meteorological Products IODC Meteosat Meteorological Products AVHRR Polar Winds - Metop-A AVHRR Polar Winds - Metop-B AVHRR Polar winds - Metop-C Multi-Metop Wind Products

Name: | EUMETSAT
Address: | Eumetsat-Allee 1 D-64295 Darmstadt Germany
Telephone: | +49 6151 807 3660/3770
Fax: | +49 6151 807 3790
E-mail: | ops@eumetsat.int
Internet: | www.eumetsat.int

Contact Information for Further M-BInformation: ESPC Operations at ESPCOperations@noaa.gov and 301-817-3880. M-BM-BM-B

This message was sent by ESPC.Notification@noaa.gov. You have been sent this and other notifications because you have opted in to receive it. If for any reason, you wish to unsubscribe, please contact ESPC Help Desk at ESPCOperations@noaa.gov or (301) 817-3880. Please note: it may take up to two business days to process your unsubscribe request.

You are receiving this email because you are subscribed to our User Notification Service (UNS). You can modify your UNS subscriptions or unsubscribe at any time via our UNS web interface (login to our Earth Observation Portal required).
Any email message from EUMETSAT is sent in good faith but shall neither be binding nor construed as constituting a commitment by EUMETSAT, except where provided for in a written agreement or contract or if explicitly stated in the email. Please note that any views or opinions presented in this email are solely those of the sender and do not necessarily represent those of EUMETSAT. This message and any attachments are intended for the sole use of the addressee(s) and may contain confidential and privileged information. Any unauthorised use, disclosure, dissemination or distribution (in whole or in part) of its contents is not permitted. If you received this message in error, please notify the sender and delete it from your system.